**4.Write an assembly language program for subtracting two 16-bit datausing 8086 processor.**

LHLD 2050

XCHG

LHLD 2052

MVI C,00

MOV A,E

SUB L

STA 2054

MOV A,D

SBB H

STA 2055

HLT